{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["FR->ANG","ANG->FR"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"FR->ANG","index":0,"n_rows":73,"n_cols":6,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"français","anglais","domaine","sous-domaine"]
[null,null,"abaque","nomogram","mathématiques",""]
[null,null,"ajustement d'une courbe","curve fitting","mathématiques",""]
[null,null,"ajuster","fit","mathématiques",""]
[null,null,"assainissement","sanitation","eau","traitement des eaux usées"]
[null,null,"averse","shower","eau","hydrologie"]
[null,null,"bassin de rétention","retarding basin","eau","gestion des eaux"]
[null,null,"bassin de retenue","reservoir","eau","gestion des eaux"]
[null,null,"bassin versant","catchment","eau","hydrologie"]
[null,null,"champs d'épandage","sewage farm","eau","traitement des eaux usées"]
[null,null,"circulaire","service instruction","gestion",""]
[null,null,"coefficient de frottement","friction coefficient","eau","hydrologie"]
[null,null,"collecteur","collector","eau","gestion des eaux"]
[null,null,"corrélation","correlation","mathématiques","statistique"]
[null,null,"débit de pointe","peak discharge","eau","hydrologie"]
[null,null,"débit de projet","design discharge","eau","hydrologie"]
[null,null,"déversement","overflow","eau","hydrologie"]
[null,null,"déversoir d'orage","storm overflow","eau","gestion des eaux"]
[null,null,"drainage","drainage","eau","gestion des eaux"]
[null,null,"eau de surface","surface water","eau","hydrologie"]
[null,null,"eau fluviale","river water","eau","hydrologie"]
[null,null,"eau potable","drinking water","eau",""]
[null,null,"eau pluviale","rain water","eau","hydrologie"]
[null,null,"eaux stagnantes","stagnant water","eau",""]
[null,null,"eaux usées domestiques","grey water","eau","traitement des eaux usées"]
[null,null,"eaux usées industrielles","industrial wastewater","eau","traitement des eaux usées"]
[null,null,"eaux vannes","black water","eau","traitement des eaux usées"]
[null,null,"écoulement à surface libre","open channel flow","eau","gestion des eaux"]
[null,null,"évaporation","evaporation","eau","hydrologie"]
[null,null,"évapotranspiration","evapotranspiration","eau","hydrologie"]
[null,null,"formule de Chézy","Chézy formula","eau","hydrologie"]
[null,null,"hauteur de pluie","rainfall","eau","hydrologie"]
[null,null,"hydrogramme","hydrograph","eau","hydrologie"]
[null,null,"hyétogramme","hyetograph","eau","hydrologie"]
[null,null,"imperméable","impermeable","eau","hydrologie"]
[null,null,"infiltration","infiltration","",""]
[null,null,"intensité de pluie","rainfall intensity","eau","hydrologie"]
[null,null,"stochastique","stochastic method","mathématiques","statistiques"]
[null,null,"stochastique","stochastic","mathématiques","statistiques"]
[null,null,"temps de concentration","time of concentration","eau","hydrologie"]
[null,null,"teneur en eau","water content","physique","milieux poreux"]
[null,null,"variable","variable","mathématiques",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
[null,""]

{"sheet":"ANG->FR","index":1,"n_rows":73,"n_cols":6,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"anglais","français","domaine","sous-domaine"]
[null,null,"black water","eaux vannes","eau","traitement des eaux usées"]
[null,null,"catchment","bassin versant","eau","hydrologie"]
[null,null,"Chézy formula","formule de Chézy","eau","hydrologie"]
[null,null,"collector","collecteur","eau","gestion des eaux"]
[null,null,"correlation","corrélation","mathématiques","statistique"]
[null,null,"curve fitting","ajustement d'une courbe","mathématiques",""]
[null,null,"design discharge","débit de projet","eau","hydrologie"]
[null,null,"drainage","drainage","eau","gestion des eaux"]
[null,null,"drinking water","eau potable","eau",""]
[null,null,"evaporation","évaporation","eau","hydrologie"]
[null,null,"evapotranspiration","évapotranspiration","eau","hydrologie"]
[null,null,"fit","ajuster","mathématiques",""]
[null,null,"friction coefficient","coefficient de frottement","eau","hydrologie"]
[null,null,"grey water","eaux usées domestiques","eau","traitement des eaux usées"]
[null,null,"hydrograph","hydrogramme","eau","hydrologie"]
[null,null,"hyetograph","hyétogramme","eau","hydrologie"]
[null,null,"impermeable","imperméable","eau","hydrologie"]
[null,null,"industrial wastewater","eaux usées industrielles","eau","traitement des eaux usées"]
[null,null,"infiltration","infiltration","",""]
[null,null,"nomogram","abaque","mathématiques",""]
[null,null,"open channel flow","écoulement à surface libre","eau","gestion des eaux"]
[null,null,"overflow","déversement","eau","hydrologie"]
[null,null,"peak discharge","débit de pointe","eau","hydrologie"]
[null,null,"rain water","eau pluviale","eau","hydrologie"]
[null,null,"rainfall","hauteur de pluie","eau","hydrologie"]
[null,null,"rainfall intensity","intensité de pluie","eau","hydrologie"]
[null,null,"reservoir","bassin de retenue","eau","gestion des eaux"]
[null,null,"retarding basin","bassin de rétention","eau","gestion des eaux"]
[null,null,"river water","eau fluviale","eau","hydrologie"]
[null,null,"sanitation","assainissement","eau","traitement des eaux usées"]
[null,null,"service instruction","circulaire","gestion",""]
[null,null,"sewage farm","champs d'épandage","eau","traitement des eaux usées"]
[null,null,"shower","averse","eau","hydrologie"]
[null,null,"stagnant water","eaux stagnantes","eau",""]
[null,null,"stochastic","stochastique","mathématiques","statistiques"]
[null,null,"stochastic method","stochastique","mathématiques","statistiques"]
[null,null,"storm overflow","déversoir d'orage","eau","gestion des eaux"]
[null,null,"surface water","eau de surface","eau","hydrologie"]
[null,null,"time of concentration","temps de concentration","eau","hydrologie"]
[null,null,"variable","variable","mathématiques",""]
[null,null,"water content","teneur en eau","physique","milieux poreux"]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
[null,null,"","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
["","","",""]
[null,""]